CALCUTTA METRO RAILWAY (TEMPORARY PROVISIONS) GENERAL RULES, 1984
22nd October, 1984
In exercise of the powers conferred by Sec. 47 of the Indian Railways Act, 1890 (9 of 1890)read with Sec. 18 of the Calcutta Metro Railway (Operation and Maintenance) Temporary Provisions Ordinance, 1984, and in supersession of the Indian Railways (Open Lines) General Rules, 1976, in so far as they relate to the Calcutta Metro Railway the Central Government hereby make the following rules, namely:


CHAPTER 01: PRELIMINARY

RULE 01.3: CLASSIFICATION OF STATIONS
- (1) Stations shall, for the purpose of these rules, be divided into two categories-block stations and non-block stations;
(2) Block Station, are those at which the Driving Motorman must obtain an authority to proceed under the system of working to enter the block section with his train;
(3) Non-block stations are stopping places situated between consecutive block stations and do not form the boundary of any block-section.


CHAPTER 02: RULES APPLYING TO METRO RAILWAY SERVANTS GENERALLY

RULE 02.11: DUTY FOR SECURING SAFETY
- (1) Every Metro Railway servant shall-
(a) see that every exertion is made for ensuring the safety of the public;
(b) promptly report to his superior any occurrence affecting the safe or proper working of the Metro Railway which may come to his notice; and
(c) render on demand all possible assistance in the case of an accident or obstruction.
(2) Every Metro Railway servant who observes-
(a) any defective signal;
(b) any obstruction, failure or threatened failure of any part of the way or works;
(c) anything wrong with a train; or
(d) any unusual circumstances likely to interfere with the safe running of trains, or the safety of the public: shall take such immediate steps, as the circumstances of the case may demand, to prevent, accident, and where necessary, advise the Traffic Controller or the nearest Station Master by the quickest possible means.


CHAPTER 03: SIGNALS
A.GENERAL PROVISIONSB.DESCRIPTION OF FIXED SIGNALC.EQUIPMENT OF SIGNALSD.WORKING OF SIGNALS AND POINTSE.HAND SIGNALS

RULE 03.38: REPORTING OF DEFECTS IN SIGNALS
-In case Driving Motorman observe that a signal light is imperfectly visible or partially obscured, he shall report the matter to the Traffic Controller on duty who shall advise the Metro Railway servant responsible for upkeep of the signals to get it rectified immediately and also inform the Station Master concerned.


